&GLOBAL
  ELPA_PRINT
  PREFERRED_DIAG_LIBRARY ELPA
  PRINT_LEVEL LOW
  PROJECT H2O-elpa-redistribute-forced
  ! Lets print information about diagonalization
  &FM_DIAG_SETTINGS ON
    ELPA_FORCE_REDISTRIBUTE TRUE
    ! Force redistribution onto 2 processors instead of the default,
    ! which is the maximum number of CPUs that can safely be used
    ! without ELPA crashing
    ! (for 8 MPI processes the maximum is 6 for this system)
    ! For most systems, this keyword should be turned off (default)
    ! for better performance
    PARAMETER_A 2
    PARAMETER_X 4
    PRINT_FM_REDISTRIBUTE TRUE
  &END FM_DIAG_SETTINGS
&END GLOBAL

&FORCE_EVAL
  METHOD Quickstep
  &DFT
    BASIS_SET_FILE_NAME BASIS_SET
    POTENTIAL_FILE_NAME POTENTIAL
    &MGRID
      CUTOFF 100
    &END MGRID
    &QS
      EPS_DEFAULT 1.0E-8
    &END QS
    &SCF
      ADDED_MOS 1 0
      EPS_SCF 1.0E-4
      SCF_GUESS ATOMIC
    &END SCF
    &XC
      &XC_FUNCTIONAL Pade
      &END XC_FUNCTIONAL
    &END XC
  &END DFT
  &SUBSYS
    &CELL
      ABC 6.0 6.0 6.0
    &END CELL
    &COORD
      O   0.000000    0.000000   -0.065587
      H   0.000000   -0.757136    0.520545
      H   0.000000    0.757136    0.520545
    &END COORD
    &KIND H
      BASIS_SET SZV-GTH-PADE
      POTENTIAL GTH-PADE-q1
    &END KIND
    &KIND O
      BASIS_SET SZV-GTH-PADE
      POTENTIAL GTH-PADE-q6
    &END KIND
  &END SUBSYS
&END FORCE_EVAL
