# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_lri01_only_es.inp                                  37    1.0E-05               0.941247E+00
h2o_lri02_es_and_gs.inp                                37    2.0E-05               0.942152E+00
#EOF
