# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
c_1.inp                                                1    1.0E-14             -45.10384660417728
c_2.inp                                                1    1.0E-14             -45.68042106170509
c_3.inp                                                1      2e-14             -45.66762356227670
c_4.inp                                                1      3e-14             -45.66762356227670
c_5.inp                                                1      3e-14             -46.02680478900018
c_6.inp                                                1      3e-14             -45.65758013574263
c_gapw.inp                                             1      2e-13            -302.06260708591526
c_gapwxc.inp                                           1      1e-12             -45.66746891467081
cn_1.inp                                               1      6e-13             -49.27303752713806
c_dos.inp                                              1      2e-14             -45.65703654036614
#EOF
