# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
2gly_DIIS-OEP-NEB.inp                                 10      2e-10              -1.27851383602517
2gly_DIIS-NEB.inp                                     10      7e-12            -2.6272600252110601
2gly_DIIS-SD-NEB.inp                                  10      5e-10              -0.92697352461672
2gly_DIIS-SD-2.inp                                    10      1e-08            -1.0649077579087201
2gly_DIIS-DNEB.inp                                    10      8e-12            -1.9198933736066299
2gly_DIIS-SM.inp                                      10      1e-11             1.7582064129930699
#EOF
