# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_apt.inp             96     1e-06     -0.879586
h2o_apt_uks.inp         96     1e-06     -0.879582
h2o_apt_loc.inp         96     1e-06     -0.879586
h2o_apt_pbc.inp         96     1e-06     -0.938707
h2o_apt_pbc_loc.inp     96     1e-06     -0.938770
h2o_aat.inp             100    1e-06     -0.857427
#EOF
