# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
regtest-Ar-S.inp              104    4.0E-06           20.8357607201
regtest-Ar-T.inp              104    4.0E-06           20.8357607201
regtest-Ne-S.inp              104    4.0E-06           45.3245164440
#EOF
