# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
H2O_sccs_td_fft.inp                                    1    1.0E-12             -17.22606913408235
H2O_sccs_td_cd5_fg.inp                                 1    1.0E-12             -17.23638536606654
#EOF
