# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
CH2O_tddfpt_stda-s-1.inp                                   37    1.0E-05               0.349885E+00
CH2Oplus_tddfpt_stda-lsd.inp                               37    1.0E-05               0.212147E+00
CH2O_tddfpt_stda-pbe-s.inp                                 37    1.0E-05               0.125452E+00
CH2O_tddfpt_stda-pbe-s_doexchange.inp                      37    1.0E-05               0.155105E+00
CH2O_tddfpt_stda-xtb-s.inp                                 37    1.0E-05               0.150482E+00
CH2O_stda-xtb-s.inp                                        37    1.0E-05               0.779158E-01
CH2O_stda-dip.inp                                          37    1.0E-05               0.779158E-01
H2O_tddfpt_stda-pbe-s.inp                                  37    1.0E-05               0.599658E+00
H2Oplus_tddfpt_stda-pbe-lsd.inp                            37    1.0E-05               0.463329E+00
H2O_tddfpt_stda-pbe-t.inp                                  37    1.0E-05               0.595565E+00
H2O_tddfpt_stda-pbe0-s.inp                                 37    1.0E-05               0.637391E+00
H2O_tddfpt_stda-pbe0-t.inp                                 37    1.0E-05               0.633489E+00
H2O_tddfpt_stda-s-1.inp                                    37    1.0E-05               0.173021E+00
NO_tddfpt_stda-s-1.inp                                     37    1.0E-05               0.375613E+00
water_xTB.inp                                              37    2.0E-05               0.125917E+00
water_xTBi_NTO.inp                                         37    2.0E-05               0.125917E+00
#EOF
