# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
NO2-EPR-1.inp                                         20      1e-01         -0.0023532400000000000
NO2-EPR-2.inp                                         20      2e-01         -0.0013230200000000002
NO2-EPR-3.inp                                         20      4e-01         -0.0012350000000000001
#EOF
