# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch2o_gapw_t1.inp                                       87      1e-05             0.483221735787E+02
ch2o_gapw_t2.inp                                       87      1e-05             0.523034637680E+02
ch2o_gapw_t3.inp                                       87      1e-05             0.514019909196E+02
ch2o_gapw_t4.inp                                       87      1e-05             0.509623579715E+02
h2o_gapw_t5.inp                                        87      1e-05             0.107325591393E+02
h2o_gapw_t6.inp                                        87      1e-05             0.154795414458E+02
h2o_gapw_t7.inp                                        87      1e-05             0.999033988860E+01
ch2o_gapw_xc_t1.inp                                    87      1e-05             0.531344520427E+02
ch2o_gapw_xc_t2.inp                                    87      1e-05             0.522983512347E+02
ch2o_gapw_xc_t3.inp                                    87      1e-05             0.513981803741E+02
ch2o_gapw_xc_t4.inp                                    87      1e-05             0.509588648640E+02
h2o_gapw_xc_t5.inp                                     87      1e-05             0.108004306906E+02
h2o_gapw_xc_t6.inp                                     87      1e-05             0.993781535670E+01
#EOF
