# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
# tests GAPW GTH and ALL
#XAS
CO.inp                                                 1      2e-12            -113.27555193628908
CO_xastpxhh.inp                                        1      1e-10            -103.60211898340968
CO_xastpval.inp                                        1      3e-11            -113.27555193676139
CO_xastpxhh_loclist.inp                                1      2e-08            -89.944402143822472
CO_xes_core1homo0.inp                                  1      3e-10            -112.77416154443722
CO_xes_core0.5.inp                                     1      3e-10            -103.51266887220301
#EOF
