# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
h2o_f01.inp                                                1    1.0E-11             -17.14073254422469
h2o_f02.inp                                                1    1.0E-11             -17.14073254422469
#EOF
