# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_pbe0.inp                                          60      1e-05             0.411901963703
h2o_pbe0_admm.inp                                     60      1e-05             0.426369189904
#
h2o_HSE06.inp                                         60      1e-05             0.436263865396
h2o_HSE06_admm.inp                                    60      1e-05             0.381688458912
#h2o_B88_mixcl.inp                 functional B88_LR   60      1e-05             0.000000000000E+00
#h2o_B88_mixcl_admm.inp            functional B88_LR   60      1e-05             0.000000000000E+00
h2o_pbe0TC.inp                                        60      1e-05             0.430192264863
h2o_pbe0TC_admm.inp                                   60      3e-05             0.390384448833
#h2o_B88_mixcl_TC_admm.inp         functional B88_LR   60      1e-05             0.000000000000E+00
#h2o_B88_mixcl_TC.inp              functional B88_LR   60      1e-05             0.000000000000E+00
#h2o_pbe0TC_LRC.inp                functional LRC
#h2o_pbe0TC_LRC_admm.inp           functional LRC
#h2o_mgga_VV3_mixcl_admm.inp       functional mgga
#h2o_mgga_VV3_mixcl.inp            functional mgga
#EOF

