# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
h2o_a01.inp                                                1    6.0E-11             -17.24005864917290
h2o_a02.inp                                                1    6.0E-11             -17.13768744679261
h2o_a03.inp                                                1    6.0E-11             -17.20804254307528
h2o_a04.inp                                                1    6.0E-11             -17.04272708960406
#EOF
