# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
# QM/MM
wdim_scc.inp                                           1    1.0E-14            -5.77017237051011  
wdim_nonscc.inp                                        1    1.0E-14            -5.77017237051011  
wdimmc_scc.inp                                         1    1.0E-14            -5.76659939309740  
wdimmc_nonscc.inp                                      1    1.0E-14            -5.76659939309740  
epc_1.inp                                              1    1.0E-14            -5.77019903377017  
epc_2.inp                                              1    1.0E-14            -5.77017237051011  
epc_3.inp                                              1    1.0E-14            -5.77019903377017  
epc_4.inp                                              1    1.0E-14            -5.77021119370205  
fdeb_1.inp                                             0
fdeb_2.inp                                             0
fdeb_3.inp                                             0
fdeb_4.inp                                             0
fdeb_5.inp                                             0
fdeb_6.inp                                             0
fdeb_7.inp                                             0
#EOF
