# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch4-gapw-issc-1.inp                                    0
ch4-gapw-issc-2.inp                                   36      1e-05             1.1241313419141019
no-gapw-issc-1.inp                                    36      9e-05             241.12852863820481
nh3-issc-op-1.inp                                     34    1.0E-14         0.1840828423510557E+02
ch4-gapw-issc-pso-1.inp                               38      5e-05                   0.386542E+01
he-polar-1.inp                                        38    1.0E-14                   0.136258E+02
#EOF
