# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o-gapw-1.inp                                        14      4e-04             458.21300000000002
h2o-gapw-3.inp                                        14      2e-03             68.856399999999994
h2o-gapw-4.inp                                        14      1e-04             427.74799999999999
o2-gapw-uks-1.inp                                     14      4E-04             754.42700000000002
o2-gapw-uks-3.inp                                     14      4e-04             1068.3199999999999
o2-gapw-uks-4.inp                                     14      9e-03             766.18899999999996
#EOF
