# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
H2O-IP-meta.inp                                        2      2e-11            -0.171588390000E+02
acid_water_meta.inp                                    1      8e-14             -79.84585655596871
#EOF
