# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch2o_1.inp                                             1      3e-13             -22.56644338703015
ch2o_2.inp                                             1      3e-13             -22.56644338703015
ch2o_3.inp                                             1      3e-13             -59.93603129436690
ch2o_4.inp                                             1      3e-13             -59.93603129436690
ch2o_5.inp                                             1      3e-13             -22.56644338703015
ch2o_6.inp                                             1      3e-13             -59.93603129436690
ch2o_7.inp                                             1      3e-13             -22.56644338703015
ch2o_8.inp                                             1      3e-13             -22.56644338703015
ch2o_9.inp                                             1      3e-13             -22.56644338703015
# tests maybe unstable
H2_upf.inp                                             1      1e-06              -1.13501864985782 
H2O_upf.inp                                            1      5e-05             -17.11484046900296 
CH2O_upf.inp                                           1      5e-05             -22.74205305294306
#EOF
