# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
H2O-hybrid-b3lyp_libxc_uks.inp                         1      3e-14             -76.41035426581175
H2O_pbe_libxc_tddfpt-s.inp                             1      6e-14             -17.23116251470402
H2O_lda_libxc_tddfpt-s.inp                             1      2e-14             -17.13289833455457
H2O_pbe_libxc_tddfpt-t_uks.inp                         1      2e-14             -17.23116251474715
H2O-hybrid-b3lyp_libxc.inp                             1      3e-14             -76.41035426581175
H2O-hybrid-wb97mv-libxc.inp                            1      2e-14             -76.39611446074743
H2O-hybrid-cam-lda0.inp                                1      3e-14             -76.47215215214956
H2O_lda_libxc_tddfpt-t_uks.inp                         1    1.0E-14             -17.13289833455855
H2O-tpssx_libxc.inp                                    1      3e-13             -33.88300963208589
diamond_br89_libxc_uks.inp                             1      7e-14             -11.06630465114328
diamond_br89_libxc.inp                                 1      7e-14             -11.06581270880638
# tpss new input
H2O-tpss_lsd.inp                                       1      3e-13             -34.34060245665712
# wb97X2 functional parametrizations
H2O-hybrid-wb97x2lp-libxc.inp                          1      3e-8              -16.89949370057707
H2O-hybrid-wb97x2tqz-libxc.inp                         1      4e-8              -16.91942374633053
#EOF
