# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
He_nmr_full.inp                                       14      2e-05                        198.893
he2_bug_disp.inp                                      14    1.0E-14                   0.144732E+03
#EOF
