# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
# dang-chang model
H2O-dimer-dangchang.inp                                2    1.0E-14            -0.707149464407E-02
H2OandI-dangchang.inp                                  2      8e-12                 -2.64972264736
deca_cg.inp                                           11    1.0E-14             -0.710872118265617
deca_sc.inp                                           11      2e-14           -0.25277947127245998
ethanol_cg.inp                                        11    1.0E-14             -0.092377428773621
ethanol_sc.inp                                        11    1.0E-14             -0.092377428770884
nacl_cg.inp                                           11      6e-14            -160.30385418395463
nacl_sc.inp                                           11      3e-14            -160.30385418386331
quartz_cg.inp                                          2    1.0E-14             0.110910625643E+02
quartz_sc.inp                                          2    1.0E-14             0.110910625668E+02
#BMHFTD and inducible dipole damping
flibe.inp                                              2    1.0E-14            -0.117512040363E+01
fli_small1.inp                                        11    1.0E-14              1.310083443876858
fli_small2.inp                                        11    1.0E-14             -0.280532103030175
fli_small3.inp                                        11    1.0E-14             -0.204261021617205
KCl.inp                                               11    1.0E-14            -24.179348645557010
#EOF
