# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch4-ch4-gpw-vdw.inp                                   11      2e-13            -16.132333052111456
#
dftd2_t1.inp                                          33    1.0E-14              -0.00291071418172
dftd2_t2.inp                                          33    1.0E-14              -0.00000858060151
dftd2_t3.inp                                          33    1.0E-14              -0.00013165830869
dftd2_t4.inp                                          33    1.0E-14              -0.02785607360072
dftd3_t1.inp                                          33    1.0E-14              -0.00147685198763
dftd3_t2.inp                                          33    1.0E-14              -0.00006284604445
dftd3_t3.inp                                          33    1.0E-14              -0.00021588485204
#
dftd3src1.inp                                         33    1.0E-14              -0.02610167828267
dftd3src2.inp                                         33    1.0E-12              -0.01190472610032
#EOF
