# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
# QM/MM
wdim_scc.inp                                           1    1.0E-14            -4.0735502369332997
wdim_nonscc.inp                                        1    1.0E-14            -4.1049845014555002
wdimmc_scc.inp                                         1    1.0E-14              -4.07060757309577
wdimmc_nonscc.inp                                      1    1.0E-14              -4.10169797261567
epc_1.inp                                              1    1.0E-14              -4.07357205844602
epc_2.inp                                              1    1.0E-14            -4.0735502369332997
epc_3.inp                                              1    1.0E-14            -4.1050091079608704
epc_4.inp                                              1    1.0E-14            -4.0735802037711499
fdeb_1.inp                                             0
fdeb_2.inp                                             0
fdeb_3.inp                                             0
fdeb_4.inp                                             0
fdeb_5.inp                                             0
fdeb_6.inp                                             0
fdeb_7.inp                                             0
#EOF
