# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
cc1.inp                                                1    1.0E-12             -45.38964266770495
bn1.inp                                               94    1.0E-14              27
#cc2.inp                   1 1.0E-12 -45.38989062944852
#cc3.inp                   1 1.0E-12 -45.38990176407365
#cc4.inp                   1 1.0E-12 -45.38975726647867
#EOF
