# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
h2o_f18.inp                                                 1    1.0E-12             -16.66860019590990
h2o_f19.inp                                                 1    1.0E-12             -16.67209150973599
h2o_f20.inp                                                 1    1.0E-12             -16.67215317932532
h2o_f21.inp                                                 1    1.0E-12             -17.01262005246088
h2o_f22.inp                                                 1    1.0E-12             -17.13162782010438
h2o_f23.inp                                                 1    1.0E-12             -17.19069234992681
h2o_f24.inp                                                 1    1.0E-12             -17.19751728760886   
#EOF
