# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch2o-nmr-nics-1.inp                                   15    4.0E-03             1896.4400000000001
h2o-nmr-nics-1.inp                                    15    4.0E-03                   0.624978E+02
no-gapw-nics.inp                                      15    1.0E-03             16514.400000000001
#EOF
