# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_dipole.inp                                        86      1e-05             0.908927636669E+00
h2o_polar.inp                                         87      1e-05             0.166347691437E+02
h2o_pdip.inp                                          86      1e-05             0.961018561809E+00
h2o_periodic.inp                                      87      1e-05             0.139741440657E+02
h2o_gga.inp                                           87      1e-05             0.165143521103E+02
h2o_gapw.inp                                          87      1e-05             0.170608453409E+02
h2o_gapw_xc.inp                                       87      1e-05             0.170656058892E+02
#EOF
