# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
# LRIGPW
2H2O_dpa_1.inp                                         1      5e-07             -34.38600444246472
2H2O_dpa_2.inp                                         1      5e-07             -34.38595551085087
2H2O_dpa_3.inp                                         1      5e-08             -34.38555829255533
2H2O_dpa_4.inp                                         1      5e-08             -34.32111657805251
2H2O_dpa_5.inp                                         1      5e-08             -34.38555820284390
2H2O_dpa_6.inp                                         1      5e-08             -34.32111650834393
#EOF
