# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
test-shrt.inp                                          0
w3-filter.inp                                          1    8.0E-13             -51.14051793253244
w3-filter-2.inp                                        1      7e-14             -78.30555080313505
#EOF
