# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch2o_t01.inp                              86    1.0E-12               0.712276774819E+00
ch2o_t02.inp                              86    1.0E-12               0.712276774819E+00
ch2o_t03.inp                              86    1.0E-12               0.755534217819E+00
ch2o_t04.inp                              86    1.0E-12               0.718756134707E+00
#EOF
