# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
# QM/MM
Cu-H2-qmmm-image-1.inp                                 1      4e-12              -1.11673069976103
Cu-H2-qmmm-image-1-gpw.inp                             1      4e-12              -1.11673069976103
Cu-H2-qmmm-image-2.inp                                 1      4e-12              -1.15440438005054
Cu-H2-qmmm-image-3.inp                                 1      4e-12              -1.11673069976121
Cu-H2-qmmm-image-4.inp                                 1      2e-13              -1.11520145054562
#EOF
