# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_lri.inp                                           87      1e-05             0.222165614960E+02
h2o_pade_fd.inp                                       87      1e-05             0.168333363169E+02
h2o_hfx.inp                                           87      1e-05             0.106990197203E+02
h2o_hfx_admm.inp                                      87      1e-05             0.153251090463E+02
h2o_admm_gapw.inp                                     87      1e-05             0.108571964857E+02
h2o_admm_x.inp                                        87      1e-05             0.108790445340E+02
#EOF
