# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
2gly_IT-NEB.inp                                       10      4e-11           -0.25218198664331998
2gly_IT-NEB-res.inp                                   10      7e-12               0.38518828458623
#EOF
