# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
H2O-chi-gpw-1.inp                                     16      1e-03                   0.212696E+03
H2O-chi-gpw-2.inp                                     16      1e-03                   0.212696E+03
O2-uks-chi-gpw-1.inp                                  16      5e-04                        102.375
O2-uks-chi-gpw-2.inp                                  16      5e-04                        102.375
#EOF
