# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_check1.inp                                         86      1e-08             0.908927636671E+00    
h2o_check2.inp                                         82      1e-06             0.00000058
#
h2o_dip40.inp                                           0
h2o_dip41.inp                                           0
h2o_dip42.inp                                           0
h2o_dip43.inp                                           0
ch2o_dip44.inp                                          0
ch2o_dip45.inp                                          0
ch2o_dip46.inp                                          0
ch2o_dip47.inp                                          0
h2o_xc_dip40.inp                                        0
h2o_xc_dip41.inp                                        0
h2o_xc_dip42.inp                                        0
h2o_xc_dip43.inp                                        0
ch2o_xc_dip44.inp                                       0
ch2o_xc_dip45.inp                                       0
ch2o_xc_dip46.inp                                       0
ch2o_xc_dip47.inp                                       0
#EOF
