# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_f01_coulomb_only.inp                 1    1.0E-11              -17.13968888100846
ch2o_f01_pbe_gapwxc.inp                  1    1.0E-11              -16.99417766936085
ch2o_f01_pbe.inp                         1    1.0E-11              -16.98005256434762
ch2o_f02_coulomb_only.inp                1    1.0E-11              -12.74156401757076
h2o_f01_coulomb_only.inp                 37    1.0E-4              0.101128E+01
ch2o_f01_pbe_gapwxc.inp                  37    1.0E-4              0.138361E+00
ch2o_f01_pbe.inp                         37    1.0E-4              0.145756E+00
ch2o_f02_coulomb_only.inp                37    1.0E-4              0.202091E+00
#ch2o_f01_pbe.inp                         8    1.0E-07     
#EOF
