# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
he-gapw-1.inp                                         14    1.0E-14                   0.100307E+03
h2o-gapw-1.inp                                        14      2e-04             458.21300000000002
ch4-gapw-1.inp                                        14      2e-03                   0.332896E+03
o2-gapw-uks-1.inp                                     14      6e-04             754.42700000000002
he-gapw-no-soft-1.inp                                 14    1.0E-14                   0.807283E-06
c2h2_list-1.inp                                       14      7e-04             287.94999999999999
no_list-1.inp                                         14      1e-01              539.1900000000001
h2o-no2-selected-states-1.inp                         14      2e-03             431.54700000000001
h2o-no2-selected-states-2.inp                         14      2e-01             312.52100000000002
w2_3-selected-states-1.inp                            14      9e-04             364.09399999999999
w2_3-selected-states-2.inp                            14      2e-02                   0.169809E+04
ch4-gapw-restart-1.inp                                14      2e-03                   0.332896E+03
o2-gapw-uks-restart-1.inp                             14      5e-04             754.48400000000004
#EOF
