# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
ch2o_t01.inp                              86    1.0E-12               0.108915750509E+01
ch2o_t02.inp                              86    1.0E-12               0.108915750509E+01
ch2o_t03.inp                              86    1.0E-12               0.114819181828E+01
ch2o_t04.inp                              86    1.0E-12               0.109829662200E+01
ch2o_t05.inp                              87    1.0E-12               0.226843652140E+02
ch2o_t06.inp                              87    1.0E-12               0.229761888713E+02
ch2o_t07.inp                              86    1.0E-12               0.954101834865E+00
ch2o_t08.inp                              86    1.0E-12               0.963128388956E+00
ch3br_nonbond_2.inp                        1    1.0E-12             -11.78062819229165  
ch3br_nonbond.inp                          1    1.0E-12             -11.78062802267188
ch3br_atprop_nonbond.inp                   1    1.0E-10             -11.78112909303997
#EOF
