# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
water_xTB.inp                                              37    2.0E-05               0.125917E+00
water_xTB_2.inp                                            37    2.0E-05               0.186821E+00
#EOF
