# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
2gly_B-NEB.inp                                        10      3e-11           -0.25722568775297999
2gly_CI-NEB.inp                                       10      5e-12              -0.18925537289823
2gly_EB-NEB.inp                                       10      2e-03             49.324084228911509
2gly_IT-NEB.inp                                       10      7e-12               0.38518828458623
#EOF
