# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
#
h2o_f09.inp                                                 1    1.0E-11             -17.04837819337335
h2o_f10.inp                                                 1    5.0E-11             -16.66860074430131    
h2o_f10b.inp                                                1    1.0E-11             -17.00363264930931   
h2o_f10c.inp                                                1    1.0E-11             -17.11290579606160  
h2o_f11.inp                                                 1    5.0E-08             -17.23630837940500
#EOF
