# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
h2o_ot_lwdn_on_the_fly_l1.inp                          1      5e-14             -17.13045715683762
h2o_ot_poly_on_the_fly_l1.inp                          1      6e-14             -17.13045715683761
o2_ot_lwdn_on_the_fly_l1.inp                           1      2e-13             -31.70815200232861
o2_ot_poly_on_the_fly_l1.inp                           1      2e-13             -31.70815200232861
h2o_ot_refine_3.inp                                    1      3e-14             -17.08884672065213
h2o_ot_refine_4.inp                                    1      2e-14             -17.11857283464189
o2_ot_refine_3.inp                                     1      5e-13             -31.60858514412410
o2_ot_refine_4.inp                                     1      2e-13             -31.58768162895743
h2o_ot_precond_1.inp                                   1      4e-14             -16.05766867329444
h2o_ot_precond_2.inp                                   1      4e-14             -16.06790080254975
h2o_ot_precond_3.inp                                   1      4e-14             -16.02559849783371
h2o_ot_precond_4.inp                                   1      4e-14             -15.85782186391535
#EOF
