# runs are executed in the same order as in this file
# the second field tells which test should be run in order to compare with the last available output
# e.g. 0 means do not compare anything, running is enough
#      1 compares the last total energy in the file
#      for details see cp2k/tools/do_regtest
NEB-MIXED.inp                                         10      8e-14            -25.757218922609201
2gly_IT-NEB-CV.inp                                    10      1e-06            -1.7874528752835901
2gly_IT-NEB-CV-res.inp                                10      5e-07              -1.79824935465504
UO2-2x2x2-CI-NEB-core-shell.inp                       10      1e-11            -462.84379294835571
UO2-2x2x2-CI-NEB-core-shell-res.inp                   10      5e-06            -462.84445967163998
#EOF
