<?xml version='1.0' encoding='utf-8'?>
<model>
  <materials>
    <material depletable="true" id="1" name="UOX fuel">
      <density units="g/cm3" value="10.062"/>
      <nuclide ao="4.9476e-06" name="U234"/>
      <nuclide ao="0.00048218" name="U235"/>
      <nuclide ao="0.021504" name="U238"/>
      <nuclide ao="1.0801e-08" name="Xe135"/>
      <nuclide ao="0.045737" name="O16"/>
    </material>
    <material id="2" name="Zircaloy">
      <density units="g/cm3" value="5.77"/>
      <nuclide ao="0.5145" name="Zr90"/>
      <nuclide ao="0.1122" name="Zr91"/>
      <nuclide ao="0.1715" name="Zr92"/>
      <nuclide ao="0.1738" name="Zr94"/>
      <nuclide ao="0.028" name="Zr96"/>
    </material>
    <material id="3" name="Cold borated water">
      <density units="atom/b-cm" value="0.07416"/>
      <nuclide ao="2.0" name="H1"/>
      <nuclide ao="1.0" name="O16"/>
      <nuclide ao="0.000649" name="B10"/>
      <nuclide ao="0.002689" name="B11"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="4" name="Hot borated water">
      <density units="atom/b-cm" value="0.06614"/>
      <nuclide ao="2.0" name="H1"/>
      <nuclide ao="1.0" name="O16"/>
      <nuclide ao="0.000649" name="B10"/>
      <nuclide ao="0.002689" name="B11"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="5" name="Reactor pressure vessel steel">
      <density units="g/cm3" value="7.9"/>
      <nuclide name="Fe54" wo="0.05437098"/>
      <nuclide name="Fe56" wo="0.88500663"/>
      <nuclide name="Fe57" wo="0.0208008"/>
      <nuclide name="Fe58" wo="0.00282159"/>
      <nuclide name="Ni58" wo="0.0067198"/>
      <nuclide name="Ni60" wo="0.0026776"/>
      <nuclide name="Mn55" wo="0.01"/>
      <nuclide name="Cr52" wo="0.002092475"/>
      <nuclide name="C0" wo="0.0025"/>
      <nuclide name="Cu63" wo="0.0013696"/>
    </material>
    <material id="6" name="Lower radial reflector">
      <density units="g/cm3" value="4.32"/>
      <nuclide name="H1" wo="0.0095661"/>
      <nuclide name="O16" wo="0.0759107"/>
      <nuclide name="B10" wo="3.08409e-05"/>
      <nuclide name="B11" wo="0.000140499"/>
      <nuclide name="Fe54" wo="0.035620772088"/>
      <nuclide name="Fe56" wo="0.579805982228"/>
      <nuclide name="Fe57" wo="0.01362750048"/>
      <nuclide name="Fe58" wo="0.001848545204"/>
      <nuclide name="Ni58" wo="0.055298376566"/>
      <nuclide name="Mn55" wo="0.018287"/>
      <nuclide name="Cr52" wo="0.145407678031"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="7" name="Upper radial reflector / Top plate region">
      <density units="g/cm3" value="4.28"/>
      <nuclide name="H1" wo="0.0086117"/>
      <nuclide name="O16" wo="0.0683369"/>
      <nuclide name="B10" wo="2.77638e-05"/>
      <nuclide name="B11" wo="0.000126481"/>
      <nuclide name="Fe54" wo="0.035953677186"/>
      <nuclide name="Fe56" wo="0.585224740891"/>
      <nuclide name="Fe57" wo="0.01375486056"/>
      <nuclide name="Fe58" wo="0.001865821363"/>
      <nuclide name="Ni58" wo="0.055815129186"/>
      <nuclide name="Mn55" wo="0.0184579"/>
      <nuclide name="Cr52" wo="0.146766614995"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="8" name="Bottom plate region">
      <density units="g/cm3" value="7.184"/>
      <nuclide name="H1" wo="0.0011505"/>
      <nuclide name="O16" wo="0.0091296"/>
      <nuclide name="B10" wo="3.70915e-06"/>
      <nuclide name="B11" wo="1.68974e-05"/>
      <nuclide name="Fe54" wo="0.03855611055"/>
      <nuclide name="Fe56" wo="0.627585036425"/>
      <nuclide name="Fe57" wo="0.014750478"/>
      <nuclide name="Fe58" wo="0.002000875025"/>
      <nuclide name="Ni58" wo="0.059855207342"/>
      <nuclide name="Mn55" wo="0.019794"/>
      <nuclide name="Cr52" wo="0.157390026871"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="9" name="Bottom nozzle region">
      <density units="g/cm3" value="2.53"/>
      <nuclide name="H1" wo="0.0245014"/>
      <nuclide name="O16" wo="0.1944274"/>
      <nuclide name="B10" wo="7.89917e-05"/>
      <nuclide name="B11" wo="0.000359854"/>
      <nuclide name="Fe54" wo="0.030411411144"/>
      <nuclide name="Fe56" wo="0.495012237964"/>
      <nuclide name="Fe57" wo="0.01163454624"/>
      <nuclide name="Fe58" wo="0.001578204652"/>
      <nuclide name="Ni58" wo="0.047211231662"/>
      <nuclide name="Mn55" wo="0.0156126"/>
      <nuclide name="Cr52" wo="0.124142524198"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="10" name="Top nozzle region">
      <density units="g/cm3" value="1.746"/>
      <nuclide name="H1" wo="0.035887"/>
      <nuclide name="O16" wo="0.2847761"/>
      <nuclide name="B10" wo="0.000115699"/>
      <nuclide name="B11" wo="0.000527075"/>
      <nuclide name="Fe54" wo="0.02644016154"/>
      <nuclide name="Fe56" wo="0.43037146399"/>
      <nuclide name="Fe57" wo="0.0101152584"/>
      <nuclide name="Fe58" wo="0.00137211607"/>
      <nuclide name="Ni58" wo="0.04104621835"/>
      <nuclide name="Mn55" wo="0.0135739"/>
      <nuclide name="Cr52" wo="0.107931450781"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="11" name="Top of fuel assemblies">
      <density units="g/cm3" value="3.044"/>
      <nuclide name="H1" wo="0.0162913"/>
      <nuclide name="O16" wo="0.1292776"/>
      <nuclide name="B10" wo="5.25228e-05"/>
      <nuclide name="B11" wo="0.000239272"/>
      <nuclide name="Zr90" wo="0.43313403903"/>
      <nuclide name="Zr91" wo="0.09549277374"/>
      <nuclide name="Zr92" wo="0.14759527104"/>
      <nuclide name="Zr94" wo="0.15280552077"/>
      <nuclide name="Zr96" wo="0.02511169542"/>
      <sab name="c_H_in_H2O"/>
    </material>
    <material id="12" name="Bottom of fuel assemblies">
      <density units="g/cm3" value="1.762"/>
      <nuclide name="H1" wo="0.0292856"/>
      <nuclide name="O16" wo="0.2323919"/>
      <nuclide name="B10" wo="9.44159e-05"/>
      <nuclide name="B11" wo="0.00043012"/>
      <nuclide name="Zr90" wo="0.3741373658"/>
      <nuclide name="Zr91" wo="0.0824858164"/>
      <nuclide name="Zr92" wo="0.1274914944"/>
      <nuclide name="Zr94" wo="0.1319920622"/>
      <nuclide name="Zr96" wo="0.0216912612"/>
      <sab name="c_H_in_H2O"/>
    </material>
  </materials>
  <geometry>
    <cell fill="200" id="1" region="-6 34 -35" universe="0"/>
    <cell fill="201" id="2" region="-6 35 -36" universe="0"/>
    <cell id="3" material="8" region="-7 31 -32" universe="0"/>
    <cell id="4" material="9" region="-5 32 -33" universe="0"/>
    <cell id="5" material="12" region="-5 33 -34" universe="0"/>
    <cell id="6" material="11" region="-5 36 -37" universe="0"/>
    <cell id="7" material="10" region="-5 37 -38" universe="0"/>
    <cell id="8" material="7" region="-7 38 -39" universe="0"/>
    <cell id="9" material="9" region="6 -7 32 -38" universe="0"/>
    <cell id="10" material="5" region="7 -8 31 -39" universe="0"/>
    <cell id="11" material="6" region="5 -6 32 -34" universe="0"/>
    <cell id="12" material="7" region="5 -6 36 -38" universe="0"/>
    <cell id="21" material="1" region="-1" universe="1"/>
    <cell id="22" material="2" region="1 -2" universe="1"/>
    <cell id="23" material="3" region="2" universe="1"/>
    <cell id="24" material="3" region="-3" universe="2"/>
    <cell id="25" material="2" region="3 -4" universe="2"/>
    <cell id="26" material="3" region="4" universe="2"/>
    <cell id="27" material="1" region="-1" universe="3"/>
    <cell id="28" material="2" region="1 -2" universe="3"/>
    <cell id="29" material="4" region="2" universe="3"/>
    <cell id="30" material="4" region="-3" universe="4"/>
    <cell id="31" material="2" region="3 -4" universe="4"/>
    <cell id="32" material="4" region="4" universe="4"/>
    <cell id="50" material="3" region="34 -35" universe="5"/>
    <cell fill="100" id="60" region="34 -35" universe="6"/>
    <cell id="70" material="4" region="35 -36" universe="7"/>
    <cell fill="101" id="80" region="35 -36" universe="8"/>
    <lattice id="100" name="Fuel assembly (lower half)">
      <pitch>1.26 1.26</pitch>
      <dimension>17 17</dimension>
      <lower_left>-10.71 -10.71</lower_left>
      <universes>
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 2 1 1 2 1 1 2 1 1 1 1 1 
1 1 1 2 1 1 1 1 1 1 1 1 1 2 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 2 1 1 2 1 1 2 1 1 2 1 1 2 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 2 1 1 2 1 1 2 1 1 2 1 1 2 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 2 1 1 2 1 1 2 1 1 2 1 1 2 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 2 1 1 1 1 1 1 1 1 1 2 1 1 1 
1 1 1 1 1 2 1 1 2 1 1 2 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 </universes>
    </lattice>
    <lattice id="101" name="Fuel assembly (upper half)">
      <pitch>1.26 1.26</pitch>
      <dimension>17 17</dimension>
      <lower_left>-10.71 -10.71</lower_left>
      <universes>
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 4 3 3 4 3 3 4 3 3 3 3 3 
3 3 3 4 3 3 3 3 3 3 3 3 3 4 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 4 3 3 4 3 3 4 3 3 4 3 3 4 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 4 3 3 4 3 3 4 3 3 4 3 3 4 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 4 3 3 4 3 3 4 3 3 4 3 3 4 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 4 3 3 3 3 3 3 3 3 3 4 3 3 3 
3 3 3 3 3 4 3 3 4 3 3 4 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 </universes>
    </lattice>
    <lattice id="200" name="Core lattice (lower half)">
      <pitch>21.42 21.42</pitch>
      <dimension>21 21</dimension>
      <lower_left>-224.91 -224.91</lower_left>
      <universes>
5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 
5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 
5 5 5 5 5 5 5 6 6 6 6 6 6 6 5 5 5 5 5 5 5 
5 5 5 5 5 6 6 6 6 6 6 6 6 6 6 6 5 5 5 5 5 
5 5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 5 
5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 
5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 
5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 
5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 
5 5 5 5 6 6 6 6 6 6 6 6 6 6 6 6 6 5 5 5 5 
5 5 5 5 5 6 6 6 6 6 6 6 6 6 6 6 5 5 5 5 5 
5 5 5 5 5 5 5 6 6 6 6 6 6 6 5 5 5 5 5 5 5 
5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 
5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 5 </universes>
    </lattice>
    <lattice id="201" name="Core lattice (lower half)">
      <pitch>21.42 21.42</pitch>
      <dimension>21 21</dimension>
      <lower_left>-224.91 -224.91</lower_left>
      <universes>
7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 
7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 
7 7 7 7 7 7 7 8 8 8 8 8 8 8 7 7 7 7 7 7 7 
7 7 7 7 7 8 8 8 8 8 8 8 8 8 8 8 7 7 7 7 7 
7 7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 7 
7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 
7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 
7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 
7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 
7 7 7 7 8 8 8 8 8 8 8 8 8 8 8 8 8 7 7 7 7 
7 7 7 7 7 8 8 8 8 8 8 8 8 8 8 8 7 7 7 7 7 
7 7 7 7 7 7 7 8 8 8 8 8 8 8 7 7 7 7 7 7 7 
7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 
7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 7 </universes>
    </lattice>
    <surface coeffs="0.0 0.0 0.41" id="1" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 0.475" id="2" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 0.56" id="3" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 0.62" id="4" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 187.6" id="5" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 209.0" id="6" type="z-cylinder"/>
    <surface coeffs="0.0 0.0 229.0" id="7" type="z-cylinder"/>
    <surface boundary="vacuum" coeffs="0.0 0.0 249.0" id="8" type="z-cylinder"/>
    <surface boundary="vacuum" coeffs="-229.0" id="31" type="z-plane"/>
    <surface coeffs="-199.0" id="32" type="z-plane"/>
    <surface coeffs="-193.0" id="33" type="z-plane"/>
    <surface coeffs="-183.0" id="34" type="z-plane"/>
    <surface coeffs="0.0" id="35" type="z-plane"/>
    <surface coeffs="183.0" id="36" type="z-plane"/>
    <surface coeffs="203.0" id="37" type="z-plane"/>
    <surface coeffs="215.0" id="38" type="z-plane"/>
    <surface boundary="vacuum" coeffs="223.0" id="39" type="z-plane"/>
  </geometry>
  <settings>
    <run_mode>eigenvalue</run_mode>
    <particles>400</particles>
    <batches>5</batches>
    <inactive>0</inactive>
    <source particle="neutron" strength="1.0" type="independent">
      <space type="box">
        <parameters>-160 -160 -183 160 160 183</parameters>
      </space>
    </source>
  </settings>
  <tallies>
    <mesh id="1">
      <dimension>2 2</dimension>
      <lower_left>-182.07 -182.07</lower_left>
      <upper_right>182.07 182.07</upper_right>
    </mesh>
    <filter id="1" type="azimuthal">
      <bins>-3.14159 -1.885 -0.6283 0.6283 1.885 3.14159</bins>
    </filter>
    <filter id="2" type="mesh">
      <bins>1</bins>
    </filter>
    <filter id="3" type="cellborn">
      <bins>10 21 22 23</bins>
    </filter>
    <filter id="4" type="delayedgroup">
      <bins>1 2 3 4 5 6</bins>
    </filter>
    <filter id="5" type="energy">
      <bins>0.0 0.253 1000.0 1000000.0 20000000.0</bins>
    </filter>
    <filter id="6" type="energyout">
      <bins>0.0 0.253 1000.0 1000000.0 20000000.0</bins>
    </filter>
    <filter id="7" type="material">
      <bins>1 2 3 4</bins>
    </filter>
    <filter id="8" type="mu">
      <bins>-1.0 -0.5 0.0 0.5 1.0</bins>
    </filter>
    <filter id="9" type="polar">
      <bins>0.0 0.6283 1.2566 1.885 2.5132 3.14159</bins>
    </filter>
    <filter id="10" type="legendre">
      <order>4</order>
    </filter>
    <filter cosine="particle" id="11" type="sphericalharmonics">
      <order>4</order>
    </filter>
    <filter id="12" type="universe">
      <bins>1 2 3 4 6 8</bins>
    </filter>
    <filter id="15" type="collision">
      <bins>1 2 5 3 6</bins>
    </filter>
    <filter id="13" type="cell">
      <bins>10 21 22 23 60</bins>
    </filter>
    <filter id="14" type="cell">
      <bins>21 22 23 27 28 29 60</bins>
    </filter>
    <tally id="1">
      <filters>1</filters>
      <scores>flux</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="2">
      <filters>1</filters>
      <scores>flux</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="3">
      <filters>1 2</filters>
      <scores>flux</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="4">
      <filters>3</filters>
      <scores>total</scores>
    </tally>
    <tally id="5">
      <filters>4</filters>
      <nuclides>U235 O16 total</nuclides>
      <scores>delayed-nu-fission decay-rate</scores>
    </tally>
    <tally id="6">
      <filters>5</filters>
      <scores>total</scores>
    </tally>
    <tally id="7">
      <filters>6</filters>
      <scores>scatter</scores>
    </tally>
    <tally id="8">
      <filters>5 6</filters>
      <scores>scatter nu-fission</scores>
    </tally>
    <tally id="9">
      <filters>7</filters>
      <scores>total</scores>
    </tally>
    <tally id="10">
      <filters>8</filters>
      <scores>scatter nu-scatter</scores>
    </tally>
    <tally id="11">
      <filters>8 2</filters>
      <scores>scatter nu-scatter</scores>
    </tally>
    <tally id="12">
      <filters>9</filters>
      <scores>flux</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="13">
      <filters>9</filters>
      <scores>flux</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="14">
      <filters>9 2</filters>
      <scores>flux</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="15">
      <filters>10</filters>
      <scores>scatter nu-scatter</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="16">
      <filters>11</filters>
      <scores>scatter nu-scatter flux total</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="17">
      <filters>11</filters>
      <scores>flux total</scores>
      <estimator>collision</estimator>
    </tally>
    <tally id="18">
      <filters>11</filters>
      <scores>flux total</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="19">
      <filters>12</filters>
      <scores>total</scores>
    </tally>
    <tally id="30">
      <filters>15</filters>
      <scores>scatter</scores>
    </tally>
    <tally id="20">
      <filters>13</filters>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="21">
      <filters>13</filters>
      <nuclides>U235 O16 total</nuclides>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="22">
      <filters>13</filters>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="23">
      <filters>13</filters>
      <nuclides>U235 O16 total</nuclides>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="24">
      <filters>13</filters>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>collision</estimator>
    </tally>
    <tally id="25">
      <filters>13</filters>
      <nuclides>U235 O16 total</nuclides>
      <scores>absorption delayed-nu-fission events fission inverse-velocity kappa-fission (n,2n) (n,n1) (n,gamma) nu-fission scatter elastic total prompt-nu-fission fission-q-prompt fission-q-recoverable decay-rate</scores>
      <estimator>collision</estimator>
    </tally>
    <tally id="26">
      <filters>14</filters>
      <scores>flux</scores>
      <estimator>tracklength</estimator>
    </tally>
    <tally id="27">
      <filters>14</filters>
      <scores>flux</scores>
      <estimator>analog</estimator>
    </tally>
    <tally id="28">
      <filters>14</filters>
      <scores>flux</scores>
      <estimator>collision</estimator>
    </tally>
    <tally id="29">
      <scores>H1-production H2-production H3-production He3-production He4-production heating damage-energy</scores>
    </tally>
  </tallies>
</model>
